Installing Private Ammyy Router
1.	Be sure that for private router you need to have dedicated external ip address (or correct port forwarding from external IP) and ports 80,443,8080 are free on this ip.
2.	Download the router.
-	Click on the link and in “File Download” dialog choose “Save”
-	Now choose one of your local disks and appropriate folder to save the file
-	Extract the content of the zip file and save files to your local disk
3.	Change password for remote access.
-	Open “router_settings.txt” located in the same folder as the main file,  “AMMYY_Router.exe”
-	Find the line starting with “password:”
-	Type the password instead of default password there and save the file
4.	Set ports and ip (optional).
Make sure that “router_settings.txt” contains valid ip and ports. 
A) For example if this Router is supposed to listen   80,443 and 8080 ports the config file should contain this record
	ports: 80,443,8080
(for correct working you need to leave these3  ports, but you can add more ports here)
B) If you want it to listen TCP pors only at a specific IP you need put it as well in ip:
(IP should belong to the host on which the router is running).
	ip: 209.162.202.200
If you want it to listen TCP ports at ALL IPs of your host you need to leave default value “0.0.0.0”
5.	Install the router as a service and start it.
-	Run application “AMMYY_Router.exe”
-	Open menu “Service” and click on ”Install”
-	Open menu “Service”and click on “Start”
6.	Check errors.
Check that no log files located in the same folder as the main file,  “AMMYY_Router.exe”. If you can find log file, please open it, it can contain error description.

Monitoring Ammyy Router activity and managing it remotely

-	Open web browser on local or remote computer
-	Open the url on it. This url should look like http://ip-address of the router : one of the ports listed in “router_settings.txt”. For example, http://127.0.0.1:8080 (for local computer)
-	Enter the password which you set up in the step 2 of “Installing Ammyy Router”
-	The following statistics is available for monitoring:
Parameter	Meanings	
Total connections:	The total number of opened TCP connections	
- target:	- number of clients	
- viewer:	- number of operators	
- control:	- number of web browser sessions registered on the router	
- unknown:	- number of connections with unknown intentions, either to use or to manage the router	
Sessions:	Number of pairs	
Max recv:		
Max sent:		
Bytes recv:	Number of bytes received by the router	
Bytes sent:	Number of bytes sent by the router	
Speed recv:	The current speed (for incoming stream) in bits/sec	
Speed sent:	The current speed (for outgoing stream) in bits/sec	

Also you may see per-connection statistics. For this you need to press “Refresh” button and choose the appropriate connection in the combobox. After that you can see an updated statistics below it:
Parameter	Meanings	
Bytes recv		
Recv Packets		
Send Packets		
Max Recv Packet Size		
Max Send Packet Size		
Max Queue Size		
Queue Size		

-	The parameters mentioned below can be changed:
Parameter	Meanings	
Stat with control connections	Default value is “YES”. It means that contol management’s connections don’t participate in statistics calculation.	
TCP Nagle	Default value is “NO”. Turns off/on Nagle algorithm. It’s not recommended to have it changed from the default value because of chances of a performance hit.	
Debug log	Default value is “NO”.	

All changes become effective immediately after their change in the web browser.

Using Ammyy Private Router with Ammyy Admin

On a Client computer:
Click menu “Ammyy” -> “Settings” and choose “Network” tab
Set Private Router
1) if router on other computer - "x.x.x.x:443,80,8080", where x.x.x.x - external IP address of your private router (example 91.1.2.103:443,80,8080)
2) if router on the same computer - "127.0.0.1:443,80,8080"

On an Operator computer:
Click menu “Ammyy” -> “Settings” and choose “Network” tab
1) if router on other computer - no need to change default settings
2) if router on the same computer, change settings
- Set Private Router "127.0.0.1:443,80,8080"
- Clear check-box "Request a client's router" (into “Common” tab)