Linksys, A Division of Cisco Systems, Inc.

Product:                WVC54GC v1.1 (ETSI version, RoHS compliant)

Classification:         Firmware Release History

Release Date:           7/07/06	

Last Firmware Version:    V1.21, Jul 7, 2006
__________________________________________________________________________

Version v1.19, Jul 7, 2006
- Fix: Unable to install ActiveX plugin to view video. Verisign digital signature expired.  

Version V1.20, Jun 06, 2006 
- Initial Release


Firmware Upgrade instructions:
- Download the zip file and extract the firmware file to your local PC. Make sure to remember it's location.
- Go to the WebUI of the camera (default IP: 192.168.1.115)
- Click "Setup" and login as administrator (default user name: admin / default password: admin)
- Click "Administrator" tab.  Then click "Upgrade Firmware" Button
- Browse to the firmware file you downloaded and click "Start Upgrade"
- Wait until the whole procedure is complete. Do not interrupt process!

